From file K0.S of the Coherent UNIX source code:

/ A20 may not enabled for up to 400 msec.  The proper handshake is to
/ send another command - we use 0xAE, keyboard enable - to the keyboard
/ controller and wait for its input buffer to be empty.  Then A20 should
/ be enabled.
